# USB Key Utility

##

Published: July 2017
Edition: 1
© 2014 - 2017 Hewlett Packard Enterprise Development LP

# Notices

The information contained herein is subject to change without notice. The only warranties for Hewlett Packard Enterprise products and services are set forth in the express warranty statements accompanying such products and services. Nothing herein should be construed as constituting an additional warranty. Hewlett Packard Enterprise shall not be liable for technical or editorial errors or omissions contained herein.

Confidential computer software. Valid license from Hewlett Packard Enterprise required for possession, use, or copying. Consistent with FAR 12.211 and 12.212, Commercial Computer Software, Computer Software Documentation, and Technical Data for Commercial Items are licensed to the U.S. Government under vendor's standard commercial license.

Links to third-party websites take you outside the Hewlett Packard Enterprise website. Hewlett Packard Enterprise has no control over and is not responsible for information outside the Hewlett Packard Enterprise website.

# Using the USB Key Utility

The USB Key Utility is a Windows application that copies Intelligent Provisioning or SPP contents, and other CD or DVD images to a USB flash drive. After copying data to the USB flash drive, you can run Intelligent Provisioning or SPP from the USB flash drive instead of from a CD or DVD. This process is beneficial in headless-server operations. It also simplifies the storage, transportation, and usage of the contents by allowing you to retrieve their images from the web and customize them as needed.

Installing the utility adds a shortcut in System Tools in the Programs Start menu folder.

Features

The USB Key Utility supports:

- ISO files larger than 1 GB.

- Quick Formatting on USB flash drives.

- USB flash drives up to a maximum of 32 GB. USB flash drives larger than 32 GB are not displayed in the utility.

# Prerequisites

Installing applications onto a USB flash drive requires a supported source CD, DVD, or ISO, and a USB flash drive with adequate storage space for storing the source contents. The USB Key Utility requires a USB 2.0 flash drive with a storage size larger than the media or ISO image (2 GB or greater).

NOTE:

Version 2.0 and later of the USB Key Utility does not support a 32-bit operating system.

AutoRun files

AutoRun files do not start automatically from the utility. To start an AutoRun file, double-click the `autorun.exe` file in the appropriate CD or DVD folder on the USB Key.

# Creating a bootable USB key

Installing the utility adds a shortcut in USB Key Utility program group in the Programs Start menu folder.

## Procedure

1. Double-click the USB Key Utility shortcut in the USB Key Utility folder.
2. Complete each step as presented by the application:
   1. Click Next at the splash screen.
   2. Read the End-User License Agreement, and then select Agree and click Next.
   3. Select Create a bootable USB key from CD/DVD, and then click Next.
      NOTE:

      Do not select the Add an additional CD/DVD to a bootable USB key option with SUM 6.2.0, SPP 2014.02.0, or Intelligent Provisioning 1.60 and later, which no longer support multiple-boot environments on a single device.

   4. Place the USB flash drive in an available USB port. Insert the media in the optical drive or mount the ISO image, and then click Next.
   5. Choose the drive letter of the source, choose the drive letter of the target USB flash drive, and click Next.
      TIP: If you do not see your drive key, click Rescan Target or insert a new one.
      CAUTION:

      All data on the target USB key will be deleted.

   6. Click Next on the warning message screen.

      The USB flash drive is formatted, and the source contents are copied to the USB flash drive.

   7. To display the `README.TXT` file, click Finish.
      NOTE:

      The `README.TXT` file is only displayed if the ISO has one to view.

# Adding content to a bootable USB key

The USB Key Utility supports multiple images on a single USB flash drive if there is adequate space available on the USB flash drive and you are not loading content that works with a UEFI bootloader, which does not support multiple images due to security reasons.

NOTE:

SUM 6.20, SPP 2014.02.0, and Intelligent Provisioning 1.60 and later no longer support multiple-boot environments on a single device. SUM, SPP, and Intelligent Provisioning contain signed parts that work with the UEFI boot loader. This change no longer allows for multi-boot setups on a single device, such as a USB key.

## Procedure

1. Follow the instructions for creating a bootable USB key.
2. Double-click the USB Key Utility shortcut in the USB Key Utility folder.
3. Complete each step presented by the application:
   1. Click Next at the splash screen.
   2. Select Agree, and then click Next after reading the End-User License Agreement.
   3. Select Add an additional CD/DVD to a bootable USB key, and then click Next.
   4. Place the USB flash drive in an available USB port. Insert the media into the optical drive or mount the ISO image, and then click Next.
   5. Choose the drive letter of the source, choose the drive letter of the target USB flash drive, and then click Next.
   6. Click Next on the informational screen.

      The source contents are copied to the USB flash drive.

   7. To display the `README.TXT` file, click Finish.
      NOTE:

      The `README.TXT` file is only displayed if the ISO has one to view.

4. Repeat steps 2-3 for each source media or image to be transferred to the USB key.